   ** How to install the device driver under DOS environment **

TEAC CD-ROM SETUP PROGRAM is the program to install the device driver under 
Windows. If you want to install it under DOS, please follow the instruction 
below.

1. Please install the hardware in your PC. (Refer to the Hardware Instruction)

2. Please copy the following 2 files located in the root directory of SETUP
   DISK in your Hard disk drive.
	TEAC_CDI.SYS
	CORELCDX.COM
	(Example)	COPY A:\TEAC_CDI.SYS C:\TEAC_CDI.SYS
			COPY A:\CORELCDX.COM C:\CORELCDX.COM
			(A:FLOPPY DISK C:HARD DISK DRIVE)

3. Please add the following line in your Config.sys file with using Text
   Editor (EDIT.COM for MS-DOS or E.EXE for PC-DOS etc). This statement can be 
   added in any line.
		DEVICE=C:\TEAC_CDI.SYS /D:TEAC-CDI
			* "C" is drive letter you copied TEAC_CDI.SYS

4. Please add the following line in your Autoexec.bat file with using Text 
   Editor (EDIT.COM for MS-DOS or E.EXE for PC-DOS). This statement can be 
   added in any line.
		C:\CORELCDX.COM /D:TEAC-CDI
			* "C" is drive letter you copied CORELCDX.COM

5. Remove the floppy disk from the drive after editing both Config.sys and 
   Autoexec.bat then reboot your computer.

6. The following should be displayed on the screen during boot-up

		C:\>C:\CORELCDX.COM /D:TEAC-CDI
		Corel CD-ROM Extensions for DOS version 1.15b
		Copyright (C) Corel Corporation 1992-1994
			Drive D: =Driver TEAC-CDI unit 0

		* "D" is drive letter assigned to CD-ROM Drive
		  This message means that TEAC CD-ROM drive is now activated.

	** Now the installation of TEAC CD-ROM drive is completed. In a future, 
	   when you install Windows, please run TEAC SETUP PROGRAM AGAIN.


  ** Q & A when you have a problem **

------------------------------------------------------------------------------
Q1: System will not boot if CD-ROM is daisy-chained with hard disk drive.
------------------------------------------------------------------------------
A: In this case, please make sure that hard disk drive jumper is set to MASTER 
   and CD-ROM's to SLAVE.
   Please refer to the installation manual for CD-ROM jumper setting and ask 
   hard drive manufacturer for MASTER jumper setting.
   Note: There may be the case that CD-ROM can not be daisy-chained with
         Conner drive (Conner mode).

------------------------------------------------------------------------------
Q2: System will hang without displaying anything when the device driver is 
   loaded.
------------------------------------------------------------------------------
A1:There is a possibility that TEAC device driver is having a conflict with 
   other. Please change the position of the device driver statement or remark
   the other driver which may be having a conflict with.
A2:In case that TEAC CD-56E drive is connected with non TEAC CD-ROM drive.
   Please re-install the TEAC CD-ROM address by going through 'SELECT I/O PORT'.

------------------------------------------------------------------------------
Q3: "Not Install Device Driver" message is displayed during loading the device 
   driver.
------------------------------------------------------------------------------
A1:Please make sure that Power cable and I/F cable are properly connected.
A2:Please make sure that there is no conflict with IDE card address (primary, 
   secondary, tertiary etc.) and/or interrupt.
A3:In case that CD-56E is daisy-chained with hard disk drive, please make sure
   that hard disk drive jumper is set to MASTER and CD-ROM's to SLAVE.
   Please refer to the installation manual for CD-ROM jumper setting and ask
   hard drive manufacturer for MASTER jumper setting.
A4:In case that your IDE I/O address is set to Tertiary/Quaternary, please 
   re-install the TEAC CD-ROM Software to change the address by selecting
   'SELECT I/O PORT'.
A5:There will be the case that CD-56E will not work with IDE Controller card 
   with Cache.

------------------------------------------------------------------------------
Q4: CD-56E will not be recognized by the system.
------------------------------------------------------------------------------
A: Drive names specified in Config.sys and Autoexec.bat may not be matching.
   Please make sure that each statement has "/D:TEAC-CDI"

------------------------------------------------------------------------------
Q5: CD-56E will not be recognized by the system with displaying "Not enough drive 
   letters".
------------------------------------------------------------------------------
A: There may be no more Drive letter available. Please add or edit "LASTDRIVE"
   statement so that the last drive equals one more than your current last drive.
	(Example)
		Current			New
		A:FDD			A:FDD
		B:FDD			B:FDD
		C:HDD			C:HDD
		D:HDD			D:HDD
					E:CD-ROM -> "LASTDRIVE=E"

------------------------------------------------------------------------------
Q6: Getting the display "XMS cache not installed"
------------------------------------------------------------------------------
A: Please refer to CorelCDX's document file (CORELCDX.TXT).

------------------------------------------------------------------------------
Q7: Getting the display "CDR101: Not Ready" when CD-ROM is accessed.
------------------------------------------------------------------------------
A: Please make sure that the disk is inserted in the drive or is not placed up 
   side down.

------------------------------------------------------------------------------
Q8: Getting the display "CDR103: CD-ROM not High Sierra or ISO 9660 format"
   when CD-ROM is accessed.
------------------------------------------------------------------------------
A: This message will be displayed when non-standard CD is accessed.
	(Example) Placing Audio CD and accessing it without going into CDPLAYER.

------------------------------------------------------------------------------
Q9: CD-56E will not be recognized when RAM Boost is used.
------------------------------------------------------------------------------
A: Please insert the statement of TEAC device driver before Ram Boost statement
   in your Config.sys.

------------------------------------------------------------------------------
Q10: Do I need BIOS CMOS Setup for my IDE CD-ROM ?
------------------------------------------------------------------------------
A: NO,CD-ROM is not supported by BIOS.It is different from Hard Disk Drive.
   Please select "none" for BIOS Setup of CD-ROM I/O port.

------------------------------------------------------------------------------
Q11: CD-PLAYER for Windows will not work.
------------------------------------------------------------------------------
A: To operate CD-PLAYER for Windows,[MCI]CD Audio has to be installed in Drivers
   in Control Panel.Please refer to Windows manual to install [MCI]CD Audio.

------------------------------------------------------------------------------
Q12: How can I see Photo CD ?
------------------------------------------------------------------------------
A: You have to use Photo CD access software released from Kodak,Corel or Adaptec
   to see Photo CD.

------------------------------------------------------------------------------
Q13: How can I see CD-I/Video CD ?
------------------------------------------------------------------------------
A: You need MPEG Playback Card (Ex. RealMagic) to play CD-I/Video CD/Karaoke CD.
   You can see a directory of Video CD but not of CD-I.

------------------------------------------------------------------------------
Q14: I can't play CD-I.
------------------------------------------------------------------------------
A: There are two kind of Disk.One is called CD-I which you have to use
   CD-I player and the other is CD-I Digital Video which you can play with
   CD-ROM drive and MPEG Playback Card.

------------------------------------------------------------------------------
Q15: Video CD Ver.2.0 can be played ?
------------------------------------------------------------------------------
A: It depends on your MPEG Playback Card.

------------------------------------------------------------------------------
Q16: Will CD-ROM drive work with i386 system ?
------------------------------------------------------------------------------
A: Yes,it will work with i386 but i486 or higher system is recommended to get 
   better performance.

------------------------------------------------------------------------------
Q17: How can I use CD-ROM under OS/2 ?
------------------------------------------------------------------------------
A: TEAC CD-ROM will work with the embedded ATAPI driver in OS/2 Warp Ver.3.0.

------------------------------------------------------------------------------
Q18: How can I get the device driver for Windows NT/95 ?
------------------------------------------------------------------------------
A: Please select embedded ATAPI driver in Windows NT/95.


==============================================================================
			Technical support
==============================================================================
		TEAC America Inc.
			Phone		213-727-4860
 			BBS		213-727-7660
			Fax on Demand	213-727-7629
