
NeoMagic Windows 95 Display Drivers Installation Procedure

1.  Boot Windows 95
2.  Run Control Panel and open the Display applet.  Change to the
    "Select" tab.
3.  Select "Display Type...".
4.  Select "Change...".
5.  Select "Have Disk...".
6.  Place the driver installation disk in drive A: and select "OK".
7.  Click "Okay" to install the NeoMagic MagicGraph128XD
    driver.  Click "Yes" to confirm you are installing a third-party driver.
8.  Click "Okay" on the message box dialog.  Shut down Win95 and reboot.

