July. 15, 1996


ThinkPad* Video Features for OS/2 Warp*
Version: 3.2.2

IBM ThinkPad 365 C/CS/CD/CSD/E/ED
==================================

SUMMARY OF NEW FUNCTIONS AND PROBLEM FIXES

Note: In the Changed/Fixed Item list,
      . n.n.n means diskette version (e.g. 3.2.2 means Version
        3.2.2)
      . (New) means new function or enhancement


---------------------------------------------------
 ThinkPad Video Features for OS/2 Warp
---------------------------------------------------

Release Version:
---------------

Version 3.2.1        Nov. 07, 1995   Initial Release for 365 C/CS/CD/CSD

Version 3.2.2        Jan. 16, 1996   Update Release for 365C/CS/CD/CSD.
                                     Also supports 365 E/ED.




Changed/Fixed Items:
-------------------

Version 3.2.2:

1. Modified the panel detection code to correctly identify LCD panel types.
   Added support for 1024x768 panels.
2. Corrected video problems in 640x480x16M color.


ThinkPad Video Features for OS/2 Warp Installation Procedure:
-----------------------------------------------------------------

NOTE: The ThinkPad Video Features for OS/2 Warp diskette must be labelled
      as CTDISP 1, before installing the driver.
      For labelling a diskette, go to DOS prompt and type
      LABEL A:CTDISP 1
      Press ENTER.


Before installation of this display driver, the system display should be set
to VGA mode. VGA is the default video mode enabled when OS/2 is installed.

If the current system primary display is not VGA, or if a previous version of
this driver is being used, the system should first be returned to VGA mode.
To restore VGA mode, use Selective Install and select VGA for Primary Display.
For more information on this procedure, see the section on Changing Display
Adapter Support in the OS/2 Users Guide.


To install this driver, do the following steps:

Step 1: Open an OS/2 full screen or windowed session.
Step 2: Place the ThinkPad Video Features for OS/2 Warp Diskette in drive A.

        Type A: <ENTER> to make this the default drive.

        Type INSTALL A: C:  <ENTER>

        where A: is the floppy disk drive and
        C: is the hard disk partition containing \OS2

        Once the Install Program is completed, do a system shutdown and
        reboot.

        A log of the information output during the install can be found
        in <root>:\OS2\INSTALL\CTINSTL.LOG


Step 3: Open the System Setup folder and run Selective Install to
        install the new device driver and configure the video
        system.

        Follow the instructions on the screen to set up the OS/2 display
        drivers in your system.  First, select Primary Display from the System
        Configuration Window. From the list of Primary Display Adapter Types,
        select Chips and Technologies 65545 and then select OK. Specify the
        correct source directory (A: Drive, if installing the display driver
        from the diskette drive), when prompted. Once the installation is
        complete, shutdown and restart the system for the installed changes to
        take effect.

        When the display driver is installed, it will be initialised
        for 640x480x256 display mode.




Trademarks:

 * Trademark of IBM Corporation.


---------------------------<< End of File >>----------------------------

*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*
NOTE:
** NO WARRANTY **  ANY USE BY YOU OF THE SOFTWARE IS AT YOUR OWN RISK.
THE SOFTWARE IS PROVIDED FOR USE "AS IS" WITHOUT WARRANTY OF ANY KIND.
TO THE MAXIMUM EXTENT PERMITTED BY LAW, IBM AND ITS SUPPLIERS DISCLAIM
ALL WARRANTIES OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING, WITHOUT
LIMITATION, IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A
PARTICULAR PURPOSE. IBM IS NOT OBLIGATED TO PROVIDE ANY UPDATES TO THE
SOFTWARE.

NO LIABILITY FOR CONSEQUENTIAL DAMAGES.  In no event shall IBM or its
suppliers be liable for any damages whatsoever (including, without limitation,
incidental, direct, indirect special and consequential damages, damages for
loss of business profits, business interruption, loss of business information,
or other pecuniary loss) arising out of the use or inability to use this
product, even if IBM has been advised of the possibility of such damages.
*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*-*
